**COMPARATIVE ASSESSEMENT OF WELL AND BOREHOLE WATER QUALITY INDEX IN SOKOTO METROPOLIS**

**Mahmud, A.Y.1͙**\***, Birnin-Yauri, U.A.2, Muhammad C.3, Magami, I.M.4͙**

1 Deparment of Pure and Environmental Chemistry, Usmanu Danfodiyo University, Sokoto

**2**Deparment of Pure and Environmental Chemistry, Usmanu Danfodiyo University, Sokoto

**3**Deparment of Energy and Applied Chemistry, Usmanu Danfodiyo University, Sokoto

**4**Deparment of Biology, Usmanu Danfodiyo University, Sokoto

\*Corresponding author. Email: meenoyabo@gmail.com. Tel: 234-703-3077100

**ABSTRACT**

The study focuses on the comparative assessment on the levels of some physiochemical parameters of well and borehole water collected from five locations in Sokoto metropolis to ascertain their quality index. Samples were collected randomly and analyzed using standard method of analysis. The physiochemical parameters analyzed include; pH, Turbidity, Total Dissolved Solids (TDS), Calcium (Ca2+), Magnesium (Mg2+), Chlorides (Cl-), Fluorides (F-) Sulphates (SO42+) and Nitrate (NO3-). The result of the study was subjected to Descriptive statistics and water quality index. The descriptive statistics results revealed that physicochemical parameters like pH, TDS, SO42-, and turbidity are within the WHO limit of drinking water while parameters like Ca2+, Mg2+ and Cl- were within and not within the WHO limit in some sampling locations whereas parameters like F- and NO3- were found not within the WHO limit in all the sampling locations.The result shows that both water sources were found within excellent and very good water quality index respectively which indicates that both water sources (well and borehole water) consumed within Sokoto metropolis are safe and suitable for drinking as it meets the minimum requirements of WHO standard of drinking water quality.

**Keywords:** Physicochemical, Index number, Correlation, metropolis, Quality index.

**INTRODUCTION**

Water is a major constituent of the human body necessary for physiochemical processes and thus crucial for human health and livelihood in general (Sobsey, 2012). This benefit of water is however assured if the water is safe for consumption and other uses. According to Meybeck *et al*. (2016), portable water is that which is odourless, colourless, tasteless, free from any form of contaminants and safe for consumption. In Nigeria, well and borehole water are among the significant sources of drinking water. However, these sources are not always safe for drinking because of the presence of impurities that affect the quality of water. (Amaechi, 2016). The water supply in State is inadequate to meet the needs of the population (Wright *et al.,* 2016). In Nigeria, despite the involvement of the World Bank, African Development Bank, and United Nations Children’s Educational Fund (UNICEF) to improve the quality of water for drinking, yet the assessment of safe water is still a challenge (Ajayi *et al.*, 2008). Regardless of its source, drinking water is usually subjected to safety and quality tests. Ishaku *et al.* (2011) stated that the water supply in rural areas in Nigeria is a public quality dilemma as over 70% of the households do not have access to clean drinking water. Gregory and Victor, (2018) confirmed this by reporting the need to examine issues arises from the increase in wells and boreholes dug in Nigeria and concerns regarding groundwater contamination. Oyedeji *et al.* (2009) reported violations of international water quality standards for the recommended aquifers for boreholes and wells dug. Borehole and well water are among the major alternative source of drinking water for the average Nigerian. However, reports indicated that most of these sources might not meet acceptable water quality for drinking purposes (Amaechi, 2016). As a result, the WHO, Food and Agricultural Organisation (FAO) and United States Environmental Protection Agency (USEPA) has set up standard for physiochemical and heavy metals contamination to ensure the quality and safety of potable water (USEPA, 2014; WHO, 2017; FAO, 2017). These standards are based on the physiochemical, heavy metals and microbiological constituents in water and defined with tolerable limits. Therefore, this study seeks to examine the quality index of physiochemical profile of potable (well and borehole water) across state metropolis.

**MATERIALS AND METHODS**

**Study Area**

Sokoto metropolis is located between latitude 1302‘45.60N and longitude 5014’20.40E. The metropolis has an estimated population of about 503, 256 people as of 2015 with 95.9 person per square kilometer and 3 percent growth rate annually based on 2016 population census (NPC, 2006). The Metropolis covers 16 km radius away from the reference points which comprises 4 local governments such as Sokoto south, Sokoto North, Wamakko and part of Kware local governments of Sokoto State, Nigeria with Local inhabitants mostly Hausa, Fulani and other groups such as, Yoruba, Igbo and other migrants. The predominant language is Hausa. Occupations of city dwellers include trading, commerce, domestication of animals with a reasonable proportion of the population working in private and public sectors. Population of farmers is on the decline (Jagaba *et al.,* 2018).



**Figure 1:** Map showing the study area

**Sampling**

Five sampling locations with longitude and latitude are designated as Moreh (5.273oE and 13.098oN), Gagi (5.282oE and 13.045oN), Kalambaina (5.192oE and 13.041oN), Kanwuri (5.198oE and 12.966oN) and UDUS Permanent site (5.239oE and 13.048oN). A total number of 45 water samples from wells and boreholes were collected for the analysis in the month of January, 2022. Three samples of each borehole and well water were collected 3 times in a day (morning, afternoon and evening) from fifteen (15) sampling locations. All the samples were collected in pre rinsed plastic containers to maintain the constant pH and minimize loss of sample and contamination. The pH, Temperature and conductivity were determined immediately at the point of collection and the samples were stored at a room temperature. (APHA, 2005)

**Analysis Technique**

The water quality parameters measured in the field were pH using pH meter, turbidity using turbidimeter, Total Dissolved Solids (TDS) and Sulphates was determined by gravimetry method, Chlorides and Nitrates by agentometry method, However, element such as Fluorides, Calcium and Magnesium were determined using Atomic Absorption Spectroscopy (AAS).

**Total Dissolved Solid (TDS)**

A clean platinum evaporating dish was placed in an oven set at 100 oC for one hour. Then it was placed in a desiccator to cool and it was weighed. It was then transferred into a hot plate; thoroughly mixed with 100 cm3 of the water sampleand was transferred by a means of measuring cylinder. The cylinder was rinsed several times with distilled water to make sure that all suspended materials transferred to the dish. After the sample was evaporated the dish and the residue was dried in an oven set at 103 oC for one hour, cooled in the desiccator and then reweighed (APHA, 2005).

**Sulphate**

100 cm3 of the sample was dispensed in a 250 cm3 capacity Erlenmeyer flask, 5ml conditioning reagent was added and mixed using a magnetic stirrer. A spoonful of barium chloride crystals was added while the solution was still being stirred, the turbidity was measured at 30 seconds after stirring at interval of 4minutes. A blank was prepared with no barium chloride added and the sulphate concentration was calculated using the formula:

$$\frac{mg}{L} SO4= \frac{mg SO4 x 1000 }{Vol.of sample}$$

**Chlorides**

20 ml of the water samples were pipetted in a conical flask. 1 ml of freshly prepared potassium chromate solution is added as an indicator and titrated against standard AgNO3 solution taken in the burette. The end point was reached when the colour change was observed from yellow to reddish brown colour.

**Nitrate**

This was carried out by the method described by APHA (2005). The sample was neutralized at pH 7. 100 cm3 of the sample was placed in a beaker and allow to evaporate to dryness on a water bath. The residue was dissolved using a glass rod with 2 cm3 disulphuric acid reagent and then transferred to Nessler’s tube. 6 cm3 of ammonium hydroxide (NH4OH) and EDTA was added drop-wise till the residue dissolved. A blank will also be prepared in the same way using distilled water instead of the sample. The colour development was read at 410 nm with a light path of 1 cm. The nitrate concentration was calculated using the formula bellow:

$$\frac{mg}{L}nitrate= \frac{mg nitrate x 1000 }{Vol.of sample}$$

**Analysis of Metals Using AAS**

Atomic absorption spectroscopy (AAS) was adopted for the analysis (Umar, 2010). The principle of the method is based on nebulising the solution of the sample into an air-acetylene flame where it vaporised. Ions of elements were atomised. The atoms formed absorb radiation of certain characteristics wavelength from their respective hollow cathode lamp. The measured absorbance is proportional to the amount of analyte in the sample solution. The concentrations of the elements: F-, Ca2+ and Mg2+ were measured using an atomic absorption spectrophotometer (AAnalyst 400 by Perkin Elmer, USA).

**Calibration of Atomic Absorption Spectrometry (AAS)**

The characteristic concentration check value is the concentration of element (in mg/l) that produces a signal of approximately 0.2 absorbance units under optimum conditions at the wavelength listed. By using the characteristic concentration check, the operator determined whether instrumental parameters are optimized and whether the instrument is performing up to specifications. Calibration of AAS was carried out by using an external calibration curve. The external calibration curve was prepared from solution of known concentrations of the sample element, which is also known as stock solution. High purity metal salts dissolved in high purity acids were used to make the stock solution. Working standards were diluted from the stock standard. From the selected sampling locations, three samples of each borehole and well water were collected

**Water Quality Index (WQI)**

The water quality index is a simple method used for the analysis of general quality of water. The method was proposed by Horton (1965) and Brown *et al.* (1970). To calculate this index, Horton (1965) proposed the first formula which takes into account all the parameters necessary to determine the quality of surface water and which reflects the composite influence of various important parameters for the assessment and management of the water quality. This index has been used for the first time to highlight the physio-chemical changes likely to occur and their impact on the quality of the water supply. The WQI is determined by comparing nine (9) water quality parameters measured in this study, namely; pH, Turbidity, Total Dissolved Solids (TDS), Calcium (Ca2+), Magnesium (Mg2+), Chlorides (Cl-), Fluorides (F-) Sulphates (SO4) and Nitrate (NO3-). The WQI is calculated by using the weighted arithmetic index method. This method consists of classifying water quality according to the degree of purity by using the most commonly measured water quality variables. The water quality index for the study was calculated using the formula in equation 1:

**𝑞𝑖 = 100 [(**𝑉**i-Vid)/(Si-Vid)] -------------------------------------------1**

**Vi** is the measured value of the ith parameter at a given sampling point

**Si** is the acceptable value of the ith parameter;

**Vid** is the ideal value of the ith parameter in pure water; it is equal to zero for all water parameters, except fluoride, dissolved oxygen and pH which are respectively 1.0mg / l; 14.6mg / l and 7.

The weighting (Wi) of the various water quality parameters is inversely proportional to the recommended standards for the corresponding parameters.

𝑊𝑖 **=** 𝐾 **/** 𝑆𝑖

With

**Wi** is the weight of the ith parameter;

**Si** is the acceptable value of the ith parameter;

**K** is a constant of proportionality given by the relation [Kalavathy et al., 2011]

**K = 1 / [1 / S1 + 1 / S2 +… + 1 / Sn] ----------------------2**

The IQE is determined from the relationship

𝐼𝑄𝐸 **= Σ** 𝑞𝑖 𝑊𝑖**/ Σ**𝑊𝑖 ------------------------------------3

𝑖**=1** 𝑖**=1**

The acceptable limit values used are taken from the values recommended by the WHO. They are given in Table 1 with the weightings of each parameter considered in the calculation of the WQI.

Five quality classes can be identified according to the values of the IQE water quality index.

 Table1.0 : WQI Classification range

|  |  |
| --- | --- |
| Water Quality assessment Grid | Class |
| 0-25 | Excellent quality water |
| 26-50 | Good quality water |
| 51-75 | Low quality water |
| 76-100 | Very low-quality water |
| >100 | Not potable water |

**4.0 RESULTS AND DISCUSSION**

Concentration of the selected physicochemical parameters and index value of the selected sampling locations were presented in the charts.

|  |  |
| --- | --- |
|  |  |

|  |  |
| --- | --- |
|  |  |
|  |  |

The average pH values range from (7.19 ± 0.35) to (7.69 ± 0.13) and from (6.169 ± 0.806) to (7.877 ± 0.180) for well and borehole water respectively. Hence, the pH values recorded in both water samples are within the WHO standard range for drinking water of 6.5-8.5. The values obtained in this study are compared with that of (Zacchaeus *et al*., 2020) who reported a pH range of 4.35 to 9.42 for groundwater in Sagamu and Ota areas of Ogun State, Nigeria. Generally, the pH of the samples tended to be slightly alkaline in all the five sampling locations. Although pH does not have a direct health implication on human beings but its indirect effects cannot be ignored (Adekunle *et al*., 2004).

The average Turbidity in well and borehole water samples ranged from (1.38 ± 0.20 NTU) to (2.19 ± 0.17 NTU) and from (1.200 ± 0.000 NTU) to (2.440 ± 0.496 NTU) which was below the WHO standard value of 5 NTU. This indicates that the turbidity of well and borehole water are within the recommended range and safe for consumption as it does not have much health impact. The level of turbidity obtained in this study is similar to 3.94 ± 1.52 NTU obtained by Michael *et al.* (2015) and disagrees with Reuben *et al.* (2018) who reports high turbidity level of 20.89 ± 6.23 in the analysis of river water collected from Nasarawa State.

Total Dissolve Solids (TDS) ranged from (71.31 ± 1.26 mg/l) to (732.56 ± 76.06 mg/l) concentration of TDS was observed from S5 and S1 sampling locations and from (263.444 ± 98.420mg/l) to (719.433 ± 526.316 mg/l) from S4 and S3 sampling locations from well and borehole water respectively. Therefore, the level of TDS recorded in all the sampling locations are within the WHO standard limit of 500-1500 mg/l, This support the findings of (Iroha *et al*., 2020) who reports the highest TDS level of (750.00 ± 1.80 ppm) and lowest TDS level of (89.11 ± 0.50 ppm) in borehole and river water samples from Ikwo. Reuben *et al.* (2018) in their study reported TDS level of 38.38 ± 8.240 mg/l. TDS also affect the taste and acceptability of drinking water if present at levels beyond recommended limits. Accordingly, the total dissolved solid values recorded in this study could be considered tolerable.

Concentration of Calcium (Ca2+) Concentration ranged from 54.75 to 562.31 mg/l from S5 and S1 and from 206.192 to 953.700 mg/l from S4 and S2 sampling locations from well and borehole water respectively whereas WHO recommended safe range for Ca2+in drinking water is 75-200 mg/l which indicates that only one sampling location was found within the recommended range of drinking water. The result of the study is not line with the findings of Oparochao *et al*. (2010) with calcium concentrations in the water samples ranging from 0.72 to 2.80 mg/l. The high level of calcium in the water samples could be attributed to the coming in contact with certain rocks and minerals especially limestone and gypsum when these minerals dissolved, they release

calcium and magnesium.

Magnesium (Mg2+) ranged from (37.26 ± .15 mg/l) to (382.63 ± 39.15 mg/l) values were reported from S5 and S1 sampling locations and from (140.343 ± 48.098 mg/l) to (649.296 ± 833.965 mg/l) from S4 and S2 sampling locations for well and borehole water respectively. The recommended permissible range for Mg2+ in drinking water is 30-150 mg/l which implies that very few among the sampling locations are found within the recommended range. The result of the study is not in line with Oparochao *et al*. (2010) who reported Mg2+concentration of 0.24mg/l to 1.50 mg/l which is quiet below the maximum allowable concentration (MAC).

The mean average concentration of Chloride (Cl-) varied from (66.52 ± 0.54 mg/l) to (683.18 ± 70.05 mg/l) from S5 and S1 sampling location and from (250.520 ± 85.857 mg/l) to (1158.834 ± 1488810 mg/l) from S4 and S2 sampling locations for well and borehole water respectively. This indicates that the chlorides (Cl-) level in some of the sampling locations are high whereas in other sampling locations are within the recommended range of 200-600 mg/l by WHO. High levels of Cl- are typically associated with having high total dissolved solids. Also presence of high level of Cl- is a common cause of well water pollution and also gives salty taste to water. This disproportionate the findings of Oparochao *et al.* (2010) with a mean of 10.86 ± 8.10 ppm chloride concentration which was low compared to the findings of the study.

Fluoride (F-) concentration varied from (2.17 ± 0.16 ppm) to (2.81 ± .47 ppm) from S5 and S1 sampling locations from (1.686 ± 0.889 ppm) to (3.025 ± 0.252 ppm) from S4 and S1 sampling locations for well and borehole water respectively. Therefore, the fluoride (F-) concentration in all the sampling locations on both water sources exceeds the WHO recommended range of 1-1.5 mg/l. A study conducted by Jdh et al. (2013) revealed the occurrence of fluoride in groundwater is due to weathering and leaching of fluoride-bearing minerals from rocks and sediments. Fluoride when digested in small quantities (˂0.5ppm) is beneficial in promoting dental health by reducing dental caries, whereas higher concentrations (>1.5 ppm) may cause fluorosis.

Sulphate (SO42-)concentration varied from (38.07 ± 3.45 mg/l) to (92.43 ± 0.78 mg/l) from S4 and S5 sampling locations and from (33.919 ± 12.712 mg/l) to (61.671±0.922 mg/l) from S4 and S1 sampling locations for well and borehole water respectively. The SO42- level in all of the sampling locations on both water sources are within the recommended range of 400 mg/l by WHO. The result of the study is above the findings of Elijah et al. (2021) with SO42- level ranging from 1.20 ppm to 6.90 ppm.

Average concentration of Nitrates (NO3-) was found to vary from 10.32mg/l (S1) to 86.08mg/l (S3) and from 16.184 mg/l (S3) to 72.886 mg/l (S5) while the standard concentration for NO3- issued by WHO is 10 mg/l. This indicates that the concentration of NO3- in both water sources of all the five sampling locations are higher than the WHO permissible limit for drinking water. This is similar to Elijah et al. (2021) with recorded Nitrate level ranging from 3.40 ppm to18.90 ppm.

**CONCLUSION**

The water quality index (WQI) results reveals that the water samples from all the sampling locations were within the of Excellent to very good water quality according to water quality index rating scale. For well water samples, four sampling locations: S1 to S4 was within the range of good water quality of 26-50 while one sampling location: S5 were found within the range of excellent water quality of 0-25 while for borehole water four sampling locations: S1, S2, S3 and S5 were found within the value of 26-50 (Good water quality) while one sampling location: S4 were found within the index value of 0-25 (Excellent water quality). Hence the quality of well and borehole water of Sokoto metropolis in terms of these physiochemical properties is safe for drinking and other purpose.

REFERENCES

Adekunle, I.M, Adetunji, M.T, Gbadebo, A.M.,andBanjoko, O.B. (2007). Assessment of Groundwater Quality in a Typical Rural Settlement in Southwest Nigeria. *International Journal of Environmental Research and Public Health* 4(4): 307-318.

Amaechi, F. (2016). Feasibility study report on small scale sachet water production at Isuaniocha Awka North local government area of Anambra State. Retrieved from <http://www.academia.edu/36164947>.

Elijah, A., A., Lois, R.M, Shola, E.A, Opeoluwa, O., Stanley, I.R.O. (2018) Quality Assessment of Selected Ground Water Sources Around a University Teaching Hospital Liquid Waste Treatment Plant.

FAO (Food and Agriculture Organisation) (2017). Chemical analysis manual for food and water, 5th Ed, FAO Rome. pp. 20-26.

Gregory, E & Victor, N. (2018). Impact of proliferation of borehole development projects on groundwater quality in Abia State, Nigeria. *International Journal of Biosciences and technology.* 11(2): 103-108.

Iroha, I.R., Ude, I.U., Okoronkwo, C., Kenneth,O., Okafor, C.O.O., and Akuma SO1 (2020). Comparative Assessment of Physicochemical Characteristics, Metal Levels and Anion Contents of Water from Different Aquatic Environments in Ebonyi State.journal of science and Technical research SSN: 2574 -1241.

Jagaba, M. A., Sirajo, A. I. and Abubakar, A. (2018). Assessment of the Causes and Problems Associated with Urban Sprawl in Sokoto Metropolis. *International Journal of Innovative Social Sciences & Humanities Research*. 6(1):42-47.

Jha, S.K., Singh, R.K., Damodaran, T., Mishra, V.K., Sharma, V.K., and Deepak, R. (2013). Fluroide in groundwater: Toxicological exposure and remedies. Toxucol Environ Health B Crit. Rev.

Meybeck, M., Kimstach, V. andHelmer, R. (2016).Strategies for water quality assessment. In: D. Chapman [Ed.] Water Quality Assessments: A Guide to the Use of Biota, Sediments and Water in Environmental Monitoring. 2nd edition, Chapman & Hall, London. pp. 23-57.

Michael, C.O., Johnmark, F.O., Victor, C.N. (2015). Analysis of the Physicochemical and Microbiological Quality of Imabolo Stream Water in Ankpa Urban Area of Kogi State, Nigeria. Mediterranean Journal of Social Sciences 6(S4).

Nigerian Standard for Drinking Water Quality, NSDWQ. Nigerian Industrial Standard Price group D Standards Organisation of Nigeria p. 1-30.

Oparaocha, E.T., Iroegbu, O.C., Obi, R.K. (2010). Assessment of Quality of Drinking Water Sources in the Federal University of Technology, Owerri, Imo State, Nigeria.Journal of Applied Biosciences 32: 1964-1976.

Oyedeji, O, Olutiola, P.O. and Moninuola, M. A. (2009). Microbiological quality of packaged drinking water brands marketed in Ibadan metropolis and IIe-Ife city in Southwestern Nigeria. *African Journal of Microbiological Research.* 4(1): 096-102.

Reuben, R.C., Gyar, S.D., and Aliyu, Y. (2018). Physicochemical and Microbiological Parameters of Water from Rivers in Keffi, Central Nigeria. Microbiology Research Journal International 24(3): 1-12.

Sobsey, M.D. (2012). Managing water in the home: Accelerated health gains from improved water supply. Sustainable Development and Healthy Environments. Geneva, World Health Organization, WHO/SDE/WSH/02.07, 2002.

United State Environmental Protection Agency (USEPA) (2014). USEPA drinking water guidelines. Retrieved September 8, 2015 from http://www.usepa.gov/ drinking water guidelines/data/getdata.html.

World Health organization (WHO) (2017). Guidelines for drinking water quality, WHO Press, Geneva, Switzerland 4th edition.

Wright, J., Dzodzomenyo, M., & Wardrop, N. A. (2016). Effects of sachet water consumption on exposure to microbe-contaminated drinking water: Household Survey evidence from Ghana. *International Journal of Environmental Research and Public Health*. 10(3): 390-398.

Zacchaeus O.O., Balogun A.M., Adeyemi A. (2020). Effects of I.ndustrialization on Groundwater Quality in Shagamu and Ota Indudustrial areas of Ogun state, Nigeria. *Research Article* Volume 6, ISSUE7, E04353. Available https://doi.org/10.1016/jheliyon.2020.e04353.